TIFFReadRGBATile
================

Synopsis
--------

.. highlight:: c

::

    #include <tiffio.h>

.. c:function:: int TIFFReadRGBATile(TIFF* tif, uint32_t x, uint32_t y, uint32_t* raster)

.. c:function:: int TIFFReadRGBATileExt(TIFF* tif, uint32_t col, uint32_t row, uint32_t * raster, int stop_on_error)

Description
-----------

:c:func:`TIFFReadRGBATile` reads a single tile of a tile-based image into
memory, storing the result in the user supplied RGBA *raster*.
The raster is assumed to be an array of ``TileWidth`` × ``TileLength``
32-bit entries, where ``TileWidth`` is the width of a tile
(:c:macro:`TIFFTAG_TILEWIDTH`) and ``TileLength`` is the height of a
tile (:c:macro:`TIFFTAG_TILELENGTH`).

:c:func:`TIFFReadRGBATileExt` provides the parameter `stop_on_error`.
Its behaviour is described at :doc:`TIFFReadRGBAImage`.

The *x* and *y* values are the offsets from the top left corner to the top
left corner of the tile to be read.  They must be an exact multiple of the
tile width and length.

Note that the raster is assume to be organized such that the pixel at
location
(*x*, *y*) is *raster* [ *y* × *width* + *x* ]; with the raster origin
in the *lower-left hand corner* of the tile. That is bottom to top
organization.  Edge tiles which partly fall off the image will be filled
out with appropriate zeroed areas.

Raster pixels are 8-bit packed red, green, blue, alpha samples. The macros
:c:macro:`TIFFGetR`, :c:macro:`TIFFGetG`, :c:macro:`TIFFGetB`, and
:c:macro:`TIFFGetA` should be used to access individual samples. Images
without Associated Alpha matting information have a constant Alpha of 1.0
(255).

See the :doc:`TIFFRGBAImage` page for more details on how various image
types are converted to RGBA values.

Notes
-----

:c:func:`TIFFReadRGBATile` is just a wrapper around the more general
:doc:`TIFFRGBAImage` facilities.  It's main advantage over the similar
:c:func:`TIFFReadRGBAImage` function is that for large images a single
buffer capable of holding the whole image doesn't need to be allocated,
only enough for one tile.  The :c:func:`TIFFReadRGBAStrip` function
does a similar operation for stripped images.

For general notes see
:ref:`TIFFRGBImage notes <TIFFRGBAImage_Restriction_Notes>`.

Return values
-------------

1 is returned if the image was successfully read and converted.
Otherwise, 0 is returned if an error was encountered.

Diagnostics
-----------

All error messages are directed to the :c:func:`TIFFErrorExtR` routine.

``"Sorry, can not handle %d-bit pictures"``:

  The image had ``BitsPerSample`` other than 1, 2, 4, 8, or 16.

``"Sorry, can not handle %d-channel images"``:

  The image had ``SamplesPerPixel`` other than 1, 3, or 4.

``Missing needed "PhotometricInterpretation" tag``:

  The image did not have a tag that describes how to display the data.

``No "PhotometricInterpretation" tag, assuming RGB``:

  The image was missing a tag that describes how to display it, but because it
  has 3 or 4 samples/pixel, it is assumed to be RGB.

``No "PhotometricInterpretation" tag, assuming min-is-black``:

  The image was missing a tag that describes how to display it,
  but because it has 1 sample/pixel, it is assumed to be a grayscale
  or bilevel image.

``"No space for photometric conversion table"``:

  There was insufficient memory for a table used to convert
  image samples to 8-bit RGB.

``Missing required "Colormap" tag``:

  A Palette image did not have a required ``Colormap`` tag.

``"No space for tile buffer"``:

  There was insufficient memory to allocate an i/o buffer.

``"No space for strip buffer"``:

  There was insufficient memory to allocate an i/o buffer.

``"Can not handle format"``:

  The image has a format (combination of ``BitsPerSample``,
  ``SamplesPerPixel``, and ``PhotometricInterpretation``)
  that :c:func:`TIFFReadRGBAImage` can not handle.

``"No space for B&W mapping table"``:

  There was insufficient memory to allocate a table used to map
  grayscale data to RGB.

``"No space for Palette mapping table"``:

  There was insufficient memory to allocate a table used to map data to 8-bit
  RGB.

See also
--------

:doc:`TIFFOpen` (3tiff),
:doc:`TIFFRGBAImage` (3tiff),
:doc:`TIFFReadRGBAImage` (3tiff),
:doc:`TIFFReadRGBAStrip` (3tiff),
:doc:`libtiff` (3tiff)
